{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":11,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARX-K"]
[]
[]
[]
[]
["","","","","","ARX20K2V1B","ARX20K5V1B9","ARX25K2V1B","ARX25K5V1B9","ARX35K2V1B","ARX35K5V1B9"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","mm","550","550","550","550","550","550"]
["","","","Ширина","mm","658","658","658","658","658","658"]
["","","","Глубина","mm","275","275","275","275","275","275"]
["Масса","Блок","","","кг","28","26","28","26","28","28"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)"]
["","","","Макс.","°C сух.т.","46","46","46","46","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15","-15","-15","-15","-15","-15"]
["","","","Макс.","°CWB","18","18","18","18","18","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","46","46","46","46","48","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","47","47","47","47","48","48"]
["Хладагент","Тип","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Заправка","","","кг","0.74","0.74","0.74","0.74","1.0","1.0"]
["","Заправка","","","tCO2Eq","1.5","1.5","1.5","1.5","2.1","2.1"]
["","ПГП","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","15","15","15","15","15","15"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","12","12","12","12","12","12"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Примечания","","","","","(1) - Рабочий диапазон в сочетании с ATX-J3: мин. 10°C с.т. ~ макс. 46°C с.т.","(1) - Рабочий диапазон в сочетании с ATX-J3: мин. 10°C с.т. ~ макс. 46°C с.т.","(1) - Рабочий диапазон в сочетании с ATX-J3: мин. 10°C с.т. ~ макс. 46°C с.т.","(1) - Рабочий диапазон в сочетании с ATX-J3: мин. 10°C с.т. ~ макс. 46°C с.т.","(1) - Рабочий диапазон в сочетании с ATX-J3: мин. 10°C с.т. ~ макс. 46°C с.т.","(1) - Рабочий диапазон в сочетании с ATX-J3: мин. 10°C с.т. ~ макс. 46°C с.т."]
["Стандартные аксессуары","LOT10 Energy Label","","","","","LOT10 Energy Label","","LOT10 Energy Label","","LOT10 Energy Label"]