{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":13,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B","ARXM35R5V1B","ARXM50R2V1B","ARXM50R5V1B","ARXM60R5V1B","ARXM60R2V1B","ARXM71R5V1B","ARXM71R2V1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","550","550","734","734","734","734","734","734"]
["","","","Ширина","мм","765","765","954","954","954","954","954","954"]
["","","","Глубина","мм","285","285","401","401","401","401","401","401"]
["Масса","Блок","","","кг","32","32","49.0","49.0","49.0","49.0","49.0","49.0"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","-10","-10","-10","-10 (4) (5), -10 (4) (5)","-10","-10","-10","-10"]
["","","","Макс.","°CDB","50, 46","50, 46","50, 46","50 (4), 46 (5)","46","46","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15","-15","-15"]
["","","","Макс.","°CWB","18","18","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","46","49","48.0","48.0","48.0","48.0","52.0","52.0"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","47","49","49.0","49.0","49.0","49.0","52.0","52.0"]
["Хладагент","Заправка","","","кг","0.76","0.76","1.15","1.15","1.15","1.15","1.15","1.15"]
["","Заправка","","","tCO2Eq","0.52","0.52","0.780","0.780","0.780","0.780","0.780","0.780"]
["","ПГП","","","","675","675","675.0","675.0","675.0","675.0","675.0","675.0"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20","20","30","30","30","30","30","30"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,035 (для длины труб свыше 10 м)","0,035 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","15","15","20.0","20.0","20.0","20.0","20.0","20.0"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1","1"]
["Электропитание","Частота","","","Гц","50","50","50","50","50","50","50","50"]
["Стандартные аксессуары","Drain cap","","","","","","3","3","3","3","3","3"]
["Примечания","","","","","","","","(1) - Возможно только в комбинации с CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B"]
["","","","","","","","","(2) - Возможно только в сочетании с CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB"]