{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-M / ARXM-M"]
[]
[]
[]
[]
["","","","","ATXM25M2V1B / ARXM25M2V1B","ATXM35M2V1B / ARXM35M2V1B","ATXM50M2V1B / ARXM50MV1B"]
["Холодопроизводительность","Мин.","","kW","1.3","1.4","1.7"]
["","Макс.","","kW","3.2","4.0","5.3"]
["","Ном.","","kW","2.5","3.40","5.02"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","285","416","728"]
["","EER","","","4.39","4.09","3.45"]
["","COP","","","5.00","4.04","3.79"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A"]
["","","Нагрев","","A","A","A"]
["Производительность по отоплению","Ном.","","kW","2.8","4.00","5.8"]
["","Мин.","","kW","1.3","1.4","1.7"]
["","Макс.","","kW","4.7","5.2","6.5"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]