{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CW"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BW"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.02"]
["","Hагрев","","Ном.","кВт","0.02"]
["Корпус","Цвет","","","","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","mm","295"]
["","","","Ширина","mm","798"]
["","","","Глубина","mm","189"]
["Масса","Блок","","","кг","11.5"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","11"]
["","","","Средн.","м³/мин","8.2"]
["","","","Низк.","м³/мин","6.1"]
["","","","Тихая работа","м³/мин","4.6"]
["","","Hагрев","Выс.","м³/мин","10.9"]
["","","Нагрев","Средн.","м³/мин","8.7"]
["","","Hагрев","Низк.","м³/мин","6.4"]
["","","","Тихая работа","м³/мин","4.5"]
["Уровень звуковой мощности","Охлаждение","","","дБA","57"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","39"]
["","","","Средн.","дБA","32"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","25"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","21"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","39"]
["","Нагрев","","Средн.","дБA","32"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","25"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","21"]
["Хладагент","ПГП","","","","675"]
["Подсоединение труб","Жидкость","","НД","mm","6.35"]
["","Газ","","НД","mm","9.5"]
["","Дренаж","","","","18"]
["Системы управления","Инфракрасный пульт ДУ","","","","ARC466A85"]
["","Проводной пульт дистанционного управления","","","","BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Воздушный фильтр","","","","2"]
["","Infrared remote control","","","","1"]
["","Remote controller mounting plate","","","","1"]
["","Screw bag","","","","1"]
["Электропитание","Наименование","","","","V1"]
["","Фаза","","","","1~"]
["","Частота","","","Гц","50"]
["","Напряжение","","","V","220-240"]