{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":21,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSHB-D / ERLA11-14DV3"]
[]
[]
[]
[]
["","","","","","EBSHB11P50DG / ERLA11D2V3","EBSHB11P30DG / ERLA11DAV3","EBSHB11P30DG / ERLA11D2V3","EBSHB11P50DG / ERLA11DAV3","EBSHB11P30DF / ERLA11DAV3","EBSHB11P50DF / ERLA11DAV3","EBSHB11P30DF / ERLA11D2V3","EBSHB11P50DF / ERLA11D2V3","EBSHB16P50DG / ERLA14D2V3","EBSHB16P30DG / ERLA14D2V3","EBSHB16P30DG / ERLA14DAV3","EBSHB16P50DG / ERLA14DAV3","EBSHB16P30DF / ERLA14DAV3","EBSHB16P50DF / ERLA14DAV3","EBSHB16P50DF / ERLA14D2V3","EBSHB16P30DF / ERLA14D2V3"]
["Внутренний блок","","","","","EBSHB11P50DG","EBSHB11P30DG","EBSHB11P30DG","EBSHB11P50DG","EBSHB11P30DF","EBSHB11P50DF","EBSHB11P30DF","EBSHB11P50DF","EBSHB16P50DG","EBSHB16P30DG","EBSHB16P30DG","EBSHB16P50DG","EBSHB16P30DF","EBSHB16P50DF","EBSHB16P50DF","EBSHB16P30DF"]
["Теплопроизводительность","Ном.","","","кВт","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)"]
["Входная мощность","Hагрев","","Ном.","кВт","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)"]
["COP","","","","","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)"]
["ГВС","Общие сведения","","Гарантированная нагрузка","","XL","L","L","XL","L","XL","L","XL","XL","L","L","XL","L","XL","XL","L"]
["","Среднеклимат. условия","","Класс энергоэффективности нагрева воды","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Отопление","Среднеклимат. темп. воды на выходе 55°C","Общ.","SCOP","","3.23","3.23","3.23","3.23","3.23","3.23","3.23","3.23","3.22","3.22","3.22","3.22","3.22","3.22","3.22","3.22"]
["","","","Класс сезонной эффективности отопления помещений","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Среднеклимат. темп. воды на выходе 35°C","Общ.","SCOP","","4.63","4.63","4.63","4.63","4.63","4.63","4.63","4.63","4.60","4.60","4.60","4.60","4.60","4.60","4.60","4.60"]
["","","","Класс сезонной эффективности отопления помещений","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Диапазон энергоэффективности","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Примечания","","","","","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Условие 1: охлаждение Ta 35°C - LWE 18°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Условие 2: охлаждение Ta 35°C - LWE 7°C (DT = 5°C); нагрев Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]