{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FAQ71CVEB / RZQSG71L3V1B","FAQ100CVEB / RZQSG100L9V1B"]
["Холодопроизводительность","Ном.","","kW","6.8","9.5"]
["Охлаждение помещений","SEER","","","6.05","5.61"]
["","Годовое потребление энергии","","кВтч/г","393","593"]
["","Производительность","Pрасч.","kW","6.80","9.50"]
["","Класс энергоэффективности","","","A+","A+"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","kW","6.00","6.81"]
["","SCOP/A","","","3.90","4.01"]
["","Класс энергоэффективности","","","A","A+"]
["","Годовое потребление энергии","","кВтч/г","2,155","2,378"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","1,060","1,580"]
["","EER","","","3.21","3.01"]
["","COP","","","3.61","3.41"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","B"]
["","","Нагрев","","A","B"]
["Теплопроизводительность","Ном.","","kW","7.5","10.8"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]