{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBQ71C8VEB / RZQSG71L3V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG100L9V1B","FBQ100C8VEB / RZQSG100L9V1B","FBQ50C8VEB / FBQ50C8VEB / RZQSG100L9V1B","FBQ125C8VEB / RZQSG125L9V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQSG125L9V1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQSG125L9V1B","FBQ60C8VEB / FBQ60C8VEB / RZQSG125L9V1B"]
["Холодопроизводительность","Ном.","","кВт","6.8","","9.5","","12.0"]
["Охлаждение помещений","SEER","","","5.81","5.10","5.50","5.10","5.20","4.80","4.80","4.80"]
["","Годовое потребление энергии","","кВтч/г","410","652","605","652","808","875","875","875"]
["","Производительность","Pрасч.","кВт","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Класс энергоэффективности","","","A+","B","A","B","A","B","B","B"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","6.00","7.60","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.88","3.80","4.01","3.80","3.90","3.80","3.80","3.80"]
["","Класс энергоэффективности","","","A","A","A+","A","A","A","A","A"]
["","Годовое потребление энергии","","кВтч/г","2,166","2,800","2,654","2,800","2,729","2,800","2,800","2,800"]
["Номинальная эффективность","Годовое потребление энергии","","kWh","1,035","","1,435","","1,870"]
["","EER","","","3.28","","3.31","","3.21"]
["","COP","","","3.61","","3.65","","3.51"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","","A","","A"]
["","","Нагрев","","A","","A","","B"]
["Теплопроизводительность","Ном.","","кВт","7.5","","10.8","","13.5"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]
["","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]