{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RXM-N9"]
[]
[]
[]
[]
["","","","","FCAG35AVEB / RXM35N2V1B9"]
["Холодопроизводительность","Ном.","","кВт","3.50"]
["Теплопроизводительность","Ном.","","кВт","4.20"]
["Номинальная эффективность","EER","","","3.72"]
["","COP","","","3.77"]
["","Годовое потребление энергии","","kWh","471"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A"]
["","","Нагрев","","A"]
["Охлаждение помещений","Класс энергоэффективности","","","A++"]
["","Производительность","Pрасч.","кВт","3.50"]
["","SEER","","","6.35"]
["","Годовое потребление энергии","","кВтч/г","193"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A++"]
["","Производительность","Pрасч.","кВт","3.32"]
["","SCOP/A","","","4.90"]
["","Годовое потребление энергии","","кВтч/г","948"]
["Примечания","","","","(1) - Электрические параметры см. в отдельных чертежах"]
["","","","","(2) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","(3) - Номинальные значения холодопроизводительности основаны на: температура внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м."]
["","","","","(4) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]