{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZAG-NV1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZAG100N7V1B"]
["Производительность по охлаждению","Ном.","","кВт","9.50 (1)"]
["Теплопроизводительность","Ном.","","кВт","10.8 (2)"]
["Охлаждение помещений","Класс энергоэффективности","","","A++"]
["","Производительность","Pрасч.","кВт","9.50"]
["","SEER","","","7.35"]
["","Годовое потребление энергии","","кВтч/г","452"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A++"]
["","Производительность","Pрасч.","кВт","9.52"]
["","SCOP/A","","","4.81"]
["","Годовое потребление энергии","","кВтч/г","2,771"]
["Примечания","","","","(1) - Охлаждение: T2: темп. в помещении 26,6°C сух.т., 19,4°C вл.т., темп. наружного воздуха 48°C сух.т. [БТЕ/ч/Вт]"]
["","","","","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]