{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-L"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / RXS35L2V1B","FCQG50FVEB / RXS50L2V1B","FCQG60FVEB / RXS60L2V1B"]
["Холодопроизводительность","Мин.","","kW","1.3","1.7","1.7"]
["","Макс.","","kW","4.0","5.3","5.7"]
["","Ном.","","kW","3.4","5.0","5.7"]
["Подсоединение труб","Жидкость","НД","мм","6.35","6.35","6.35"]
["","Газ","НД","мм","9.5","12.70","12.70"]
["","Дренаж","OD","мм","VP25 (внешний диам.32, внутр. диам. 25)","VP25 (внешний диам.32, внутр. диам. 25)","VP25 (внешний диам.32, внутр. диам. 25)"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","475","705","820"]
["","EER","","","3.58","3.55","3.48"]
["","COP","","","3.50","3.7","3.52"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A"]
["","","Нагрев","","B","A","B"]
["Производительность по отоплению","Ном.","","kW","4.20","6.00","7.0"]
["","Мин.","","kW","1.3","1.7","1.7"]
["","Макс.","","kW","5.2","6.0","7.0"]
["Примечания","","","","(1) - 220 В","(1) - 220 В","(1) - 220 В"]
["","","","","(2) - 230 В","(2) - 230 В","(2) - 230 В"]
["","","","","(3) - 240В","(3) - 240В","(3) - 240В"]
["","","","","(4) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(4) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(4) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(5) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(5) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(5) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]