{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQG-L8/7V1"]
[]
[]
[]
[]
["","","","","FCQHG71FVEB / RZQG71L8V1B","FCQHG100FVEB / RZQG100L8V1B","FCQHG125FVEB / RZQG125L8V1B","FCQHG140FVEB / RZQG140L7V1B"]
["Холодопроизводительность","Ном.","","кВт","6.8","9.5","12.0","13.4"]
["Охлаждение помещений","SEER","","","7.00","7.00","6.61"]
["","Годовое потребление энергии","","кВтч/г","340","475","635.401"]
["","Производительность","Pрасч.","кВт","6.80","9.50","12.00"]
["","Класс энергоэффективности","","","A++","A++","A++"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","7.60","11.30","12.66"]
["","SCOP/A","","","4.54","4.80","4.63"]
["","Класс энергоэффективности","","","A+","A++","A++"]
["","Годовое потребление энергии","","кВтч/г","2,343","3,295.833","3,829"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","830","1,075","1,500","2,000"]
["","EER","","","4.09","4.42","4.00","3.35"]
["","COP","","","4.80","4.99","4.40","4.12"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A"]
["","","Нагрев","","A","A","A"]
["Теплопроизводительность","Ном.","","кВт","7.5","10.8","13.5","15.5"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]