{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQHG100FVEB / RZQSG100L8Y1B","FCQHG125FVEB / RZQSG125L8Y1B","FCQHG140FVEB / RZQSG140L7Y1B"]
["Холодопроизводительность","Ном.","","кВт","9.5","12.0","13.4"]
["Охлаждение помещений","SEER","","","6.7","5.4"]
["","Годовое потребление энергии","","кВтч/г","497","778"]
["","Производительность","Pрасч.","кВт","9.5","12"]
["","Класс энергоэффективности","","","A++","A"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","8.03","8.03"]
["","SCOP/A","","","4.3","4.1"]
["","Класс энергоэффективности","","","A+","A+"]
["","Годовое потребление энергии","","кВтч/г","2,615","2,742"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","1,285","1,855"]
["","EER","","","3.70","3.23","3.21"]
["","COP","","","4.30","3.75","3.61"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A"]
["","","Нагрев","","A","A"]
["Теплопроизводительность","Ном.","","кВт","10.8","13.5","15.5"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]