{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-D3/D9V1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125D9V1B"]
["Холодопроизводительность","Ном.","","кВт","12.5 (3)"]
["Piping connections","Жидкость","OD","мм","9.52"]
["","Газ","НД","мм","15.9"]
["","Дренаж","OD","мм","26"]
["Space cooling","SEER","","","3.50"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","1,978"]
["","EER","","","3.16"]
["","COP","","","3.88"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","B"]
["","","Нагрев","","A"]
["Теплопроизводительность","Ном.","","кВт","14.0 (4)"]
["Примечания","","","","(1) - Класс энергопотребления: шкала от A (более энергоэффект.) до G (менее энергоэффект.)"]
["","","","","(2) - Годовое потребление энергии: на основе среднего использования в течение 500 часов ежегодной работы при полной нагрузке (номинальные условия)"]
["","","","","(3) - Охлаждение: темп. в помещении: 27°CDB, 19°CWB; темп. наружного воздуха 35°CDB; эквивалентная длина трубопроводов: 5м; перепад уровня: 0 м"]
["","","","","(4) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 5м; перепад уровня: 0 м"]
["","","","","(5) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]