{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-L3"]
[]
[]
[]
[]
["","","","","FDXS25F2VEB / RXS25L3V1B","FDXS35F2VEB / RXS35L3V1B"]
["Холодопроизводительность","Мин.","","кВт","1.3","1.4"]
["","Макс.","","кВт","3.0","3.8"]
["","Ном.","","кВт","2.4 (2)","3.4 (2)"]
["Подсоединения труб","Жидкость","НД","мм","6.35","6.35"]
["","Газ","НД","мм","9.5","9.5"]
["","Дренаж","НД","мм","VP20 (внешний диам.26, внутр. диам. 20)","VP20 (внешний диам.26, внутр. диам. 20)"]
["Номинальная эффективность","Годовое потребление энергии","","kWh","321","574"]
["","EER","","","3.74 (1)","2.96 (1)"]
["","COP","","","4.00 (1)","3.48 (1)"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","B"]
["","","Нагрев","","A","A"]
["Теплопроизводительность","Ном.","","кВт","3.2 (2)","4.0 (2)"]
["","Мин.","","кВт","1.3","1.4"]
["","Макс.","","кВт","4.5","5.0"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]