{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":10,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG71L9V1B","FDXS35F2VEB / FDXS35F2VEB / RZQG71L9V1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L9V1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG100L9V1B","FDXS60F2VEB / FDXS60F2VEB / RZQG125L9V1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQG125L9V1B"]
["Space cooling","SEER","","","4.80","4.80","5.10","5.10","5.10","5.10"]
["","Годовое потребление энергии","","кВтч/г","496","496","652","652","824","824"]
["","Производительность","Pрасч.","кВт","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Класс энергоэффективности","","","B","B","B","B","B","B"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","6.00","6.00","10.74","10.74","12.71","11.30"]
["","SCOP/A","","","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Класс энергоэффективности","","","A","A","A","A","A","A"]
["","Годовое потребление энергии","","кВтч/г","2,211","2,211","3,957","3,957","4,683","4,164"]
["Примечания","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]