{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG125L8Y1B","FFA60A2VEB9 / FFA60A2VEB9 / RZQG125L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG71L8Y1B"]
["Диапазон энергоэффективности","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Производительность по охлаждению","Ном.","","kW","","","","","","","","6.80","6.80","6.80"]
["Охлаждение помещений","SEER","","","","","","","","","","5.10","5.10","5.10"]
["","Годовое потребление энергии","","кВтч/г","","","","","","","","467","467","467"]
["","Производительность","Pрасч.","kW","","","","","","","","6.80","6.80","6.80"]
["","Класс энергоэффективности","","","","","","","","","","A","A","A"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","kW","","","","","","","","6.00","6.00","6.00"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80"]
["","Класс энергоэффективности","","","","","","","","","","A","A","A"]
["","Годовое потребление энергии","","кВтч/г","","","","","","","","2,211","2,211","2,211"]
["Номинальная эффективность","EER","","","","","","","","","","3.38","3.38","3.38"]
["Примечания","","","","","","","","","","","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Номинальные значения холодопроизводительности основаны на: температура внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м.","(1) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","","","","","","","(2) - Электрические параметры см. в отдельных чертежах","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м.","(2) - Электрические параметры см. в отдельных чертежах"]
["","","","","","","","","","","","","(3) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","","","","","","","","(4) - Электрические параметры см. в отдельных чертежах"]