{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CS"]
[]
[]
[]
[]
["","","","","","FTXA20C2V1BS","FTXA25C2V1BS","FTXA35C2V1BS","FTXA42C2V1BS","FTXA50C2V1BS"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.02","0.022","0.023","0.028","0.030"]
["","Hагрев","","Ном.","кВт","0.02","0.02","0.22","0.036","0.039"]
["Корпус","Цвет","","","","Серебристый","Серебристый","Серебристый","Серебристый","Серебристый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","295","295","295","295","295"]
["","","","Ширина","мм","798","798","798","798","798"]
["","","","Глубина","мм","189","189","189","189","189"]
["Масса","Блок","","","кг","11.5","11.5","11.5","11.5","11.5"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","11","11.5","11.9","13.1","13.5"]
["","","","Средн.","м³/мин","8.2","8.6","8.6","9.8","10.4"]
["","","","Низк.","м³/мин","6.1","6.1","6.1","7.2","7.6"]
["","","","Тихая работа","м³/мин","4.6","4.6","4.6","4.6","5.2"]
["","","Hагрев","Выс.","м³/мин","10.9","11.1","11.5","14.6","15.1"]
["","","Нагрев","Средн.","м³/мин","8.7","9","9","10.5","11.1"]
["","","Hагрев","Низк.","м³/мин","6.4","6.4","6.4","7.7","8.2"]
["","","","Тихая работа","м³/мин","4.5","4.5","4.5","5.2","5.7"]
["Уровень звуковой мощности","Охлаждение","","","дБA","57","57","60","60","60"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","39","40","41","45","46"]
["","","","Средн.","дБA","32","33","33","37","39"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","25","25","25","29","31"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","19","19","19","21","24"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","39","40","41","45","46"]
["","Нагрев","","Средн.","дБA","32","33","33","37","42"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","25","25","25","29","33"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","19","19","19","21","24"]
["Хладагент","ПГП","","","","675","675","675","675","675.0"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.5","9.5","9.5","9.5","12.70"]
["","Дренаж","","","","18","18","18","18","18"]
["Системы управления","Инфракрасный пульт ДУ","","","","ARC466A85","ARC466A85","ARC466A85","ARC466A85","ARC466A85"]
["","Проводной пульт дистанционного управления","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Воздушный фильтр","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Remote controller mounting plate","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["Электропитание","Наименование","","","","V1","V1","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240","220-240","220-240"]