{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-E"]
[]
[]
[]
[]
["","","","","","FTXF20E5V1B","FTXF25E5V1B","FTXF35E5V1B","FTXF42E5V1B"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.023","0.023","0.029","0.040"]
["","Hагрев","","Ном.","кВт","0.023","0.023","0.029","0.040"]
["Корпус","Цвет","","","","Белый","Белый","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","286","286","286"]
["","","","Ширина","мм","770","770","770","770"]
["","","","Глубина","мм","225","225","225","225"]
["Масса","Блок","","","кг","8","8","8.5","9.00"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","9.8","10","11.5","12.6"]
["","","","Средн.","м³/мин","8","8","8","9"]
["","","","Низк.","м³/мин","6","6.2","6.4","6.9"]
["","","","Тихая работа","м³/мин","4.3","4.3","4.4","4.9"]
["","","Hагрев","Выс.","м³/мин","10.4","10.4","11.9","12.8"]
["","","Нагрев","Средн.","м³/мин","8.3","8.4","8.6","8.8"]
["","","Hагрев","Низк.","м³/мин","6.2","6.4","6.5","6.7"]
["","","","Тихая работа","м³/мин","5.3","5.3","5.3","5.2"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","53","54","54","59.0"]
["","Отопление","","","дБ(A)","55","55","56","59.0"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","","40","43","45.0"]
["","","","Средн.","дБ(A)","33","33","34","36.0"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","","26","27","30.0"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","","20","20","22.0"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","","40","40","44.0"]
["","Нагрев","","Средн.","дБ(A)","34","34","35","34.0"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","","28","29","28.0"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","","21","21","22.0"]
["Подсоединение труб","Жидкость","","НД","мм","6","6","6","6"]
["","Газ","","НД","мм","9.5","9.5","9.5","9.50"]
["","Дренаж","","","","18","18","18","18"]
["Системы управления","Инфракрасный пульт ДУ","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["","Проводной пульт дистанционного управления","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50"]
["","Напряжение","","","V","220-440","220-440","220-440","220-440"]
["Размеры","Блок","","Высота","мм","286"]
["Уровень звукового давления","Охлаждение","","Выс.","дБA","39"]
["","","","Низк.","дБA","25"]
["","","","Тихая работа","дБA","20"]
["","Hагрев","","Выс.","дБA","39"]
["","","","Низк.","дБA","28"]
["","","","Тихая работа","дБA","21"]