{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":14,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / RXJ-M"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / RXJ20M3V1B","FTXJ20MV1BW / RXJ20M5V1B","FTXJ20MV1BW / RXJ20M2V1B","FTXJ25MV1BW / RXJ25M2V1B","FTXJ25MV1BW / RXJ25M3V1B","FTXJ25MV1BW / RXJ25M5V1B","FTXJ35MV1BW / RXJ35M2V1B","FTXJ35MV1BW / RXJ35M5V1B","FTXJ35MV1BW / RXJ35M3V1B","FTXJ50MV1BW / RXJ50MV1B"]
["Производительность по охлаждению","Мин.","","кВт","1.30","","","","0.90"]
["","Макс.","","кВт","2.80","","","","3.30"]
["","Ном.","","кВт","2.30","2.30","2.3","2.4","2.40","2.40","3.5","3.50","","4.80"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","248","248","248","254","254","254","428","428","","716"]
["","EER","","","4.64","4.64","4.64","4.73","4.73","4.73","4.09","4.09","","3.35"]
["","COP","","","5.00","5.00","5.00","4.57","4.57","4.57","4.04","4.04","","3.65"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A","A","A","A","A","A","","A"]
["","","Нагрев","","A","A","A","A","A","A","A","A","","A"]
["Теплопроизводительность","Ном.","","кВт","2.50","2.5","2.5","3.2","3.20","3.2","4","4.0","","5.80"]
["","Мин.","","кВт","1.30","","","","0.90"]
["","Макс.","","кВт","4.30","","","","4.70"]
["Примечания","","","","(1) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(1) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","","(1) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(1) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","(1) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]
["","","","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","","","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]
["Холодопроизводительность","Мин.","","кВт","","","","","","","","","0.90"]
["","Ном.","","кВт","","","","","","","","","3.50"]
["","Макс.","","кВт","","","","","","","","","4.10"]
["Теплопроизводительность","Мин.","","кВт","","","","","","","","","0.90"]
["","Ном.","","кВт","","","","","","","","","4.00"]
["","Макс.","","кВт","","","","","","","","","5.10"]
["Номинальная эффективность","EER","","","","","","","","","","","4.09"]
["","COP","","","","","","","","","","","4.04"]
["","Годовое потребление энергии","","кВтч","","","","","","","","","428"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","","","","","","","","","A"]
["","","Нагрев","","","","","","","","","","A"]
["Охлаждение помещений","Класс энергоэффективности","","","","","","","","","","","A++"]
["","Производительность","Pрасч.","кВт","","","","","","","","","3.50"]
["","SEER","","","","","","","","","","","7.19"]
["","Годовое потребление энергии","","кВтч/г","","","","","","","","","170"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","","","","","","","","","A++"]
["","Производительность","Pрасч.","кВт","","","","","","","","","3.00"]
["","SCOP/A","","","","","","","","","","","4.60"]
["","Pdh Теплопроизводительность при -10°","","кВт","","","","","","","","","2.61"]
["","Годовое потребление энергии","","кВтч/г","","","","","","","","","913"]