{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RZAG-B"]
[]
[]
[]
[]
["","","","","FTXM35R2V1B / RZAG35B5V1B","FTXM35R5V1B / RZAG35B5V1B","FTXM60R2V1B / RZAG60B5V1B"]
["Холодопроизводительность","Мин.","","кВт","1.6","1.6","1.7"]
["","Ном.","","кВт","3.5","3.5","6"]
["","Макс.","","кВт","5","5","6.8"]
["Теплопроизводительность","Мин.","","кВт","1.4","1.4","1.6"]
["","Ном.","","кВт","4","4","7"]
["","Макс.","","кВт","5.3","5.3","7.5"]
["Номинальная эффективность","EER","","","4.3","4.3","3.5"]
["","COP","","","3.85","3.85","3.61"]
["","Годовое потребление энергии","","кВтч","407","407","857"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A"]
["","","Нагрев","","A","A","A"]
["Охлаждение помещений","Класс энергоэффективности","","","A++","A++","A++"]
["","Производительность","Pрасч.","кВт","3.5","3.5","6"]
["","SEER","","","7.7","7.7","6.9"]
["","Годовое потребление энергии","","кВтч/г","159","159","304"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A++","A++","A+"]
["","Производительность","Pрасч.","кВт","2.6","2.6","4.6"]
["","SCOP/A","","","4.6","4.6","4.35"]
["","Pdh Теплопроизводительность при -10°","","кВт","2.47","2.47","4.02"]
["","Годовое потребление энергии","","кВтч/г","790","790","1480"]
["Диапазон энергоэффективности","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]