{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-L"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RXS60L2V1B"]
["Холодопроизводительность","Мин.","","кВт","1.7"]
["","Ном.","","кВт","6.0"]
["","Макс.","","кВт","6.7"]
["Теплопроизводительность","Мин.","","кВт","1.7"]
["","Ном.","","кВт","7.0"]
["","Макс.","","кВт","8.0"]
["Номинальная эффективность","EER","","","3.02"]
["","COP","","","3.43"]
["","Годовое потребление энергии","","кВтч","995"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","B"]
["","","Нагрев","","B"]
["Подсоединения труб","Дренаж","НД","мм","18"]
["Подсоединение труб","Газ","НД","мм","12.7"]
["","Жидкость","НД","мм","6.35"]
["Охлаждение помещений","Класс энергоэффективности","","","A"]
["","Производительность","Pрасч.","кВт","6.00"]
["","SEER","","","5.58"]
["","Годовое потребление энергии","","кВтч/г","376"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A"]
["","Производительность","Pрасч.","кВт","4.80"]
["","SCOP/A","","","3.89"]
["","Годовое потребление энергии","","кВтч/г","1728"]
["Примечания","","","","(1) - 220 В"]
["","","","","(2) - 230 В"]
["","","","","(3) - 240В"]