{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BW"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BW"]
["Уровень звукового давления","Hагрев","","Выс.","дБ(A)","41"]
["","","","Средн.","дБ(A)","31"]
["","","","Тихая работа","дБ(A)","19"]
["","","","Низк.","дБ(A)","24"]
["","Охлаждение","","Средн.","дБ(A)","32"]
["","","","Тихая работа","дБ(A)","20"]
["","","","Низк.","дБ(A)","25"]
["","","","Выс.","дБ(A)","43"]
["Стандартные аксессуары","Инструкции по установке","","","","1"]
["","Руководство по эксплуатации","","","","1"]
["","Воздушный фильтр","","","","2"]
["","Пульт дистанционного управления","","","","1"]
["","Монтажная пластина пульта дистанционного управления","","","","1"]
["","Пакет для винтов","","","","1"]
["","Чехол для винтов","","","","2"]
["","Сухие батареи AAA","","","","2"]
["","Общие меры предосторожности","","","","1"]
["Хладагент","ПГП","","","","675.0"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Подсоединение труб","Жидкость","","НД","мм","6.35"]
["","Газ","","НД","мм","9.50"]
["","Дренаж","","","","18"]
["Power input","Охлаждение","","Ном.","кВт","0.023"]
["","Hагрев","","Ном.","кВт","0.022"]
["Sound power level","Охлаждение","","","дБ(A)","60"]
["","Отопление","","","дБ(A)","60"]
["Размеры","Блок","","Ширина","мм","798"]
["","","","Глубина","мм","189"]
["","","","Высота","мм","295"]
["Корпус","Цвет","","","","Белый"]
["Масса","Блок","","","kg","11.5"]
["Вентилятор","Расход воздуха","Hагрев","Выс.","м³/мин","11.5"]
["","","","Низк.","м³/мин","6.0"]
["","","","Средн.","м³/мин","8.0"]
["","","","Тихая работа","м³/мин","5.1"]
["","","Охлаждение","Низк.","м³/мин","5.7"]
["","","","Средн.","м³/мин","8.3"]
["","","","Выс.","м³/мин","11.9"]
["","","","Тихая работа","м³/мин","4.6"]
["Power supply","Фаза","","","","1~"]
["","Частота","","","Гц","50"]
["","Наименование","","","","V1"]
["","Напряжение","","","В","220-240"]
["Примечания","","","","","(1) - Охлаждение: темп. в помещении: 27°CDB, 19,0°CWB; темп. наружного воздуха 35°CDB, 24°CWB; эквивалентная длина трубопроводов: 5 м"]
["","","","","","(2) - Нагрев: темп. в помещении: 20°CDB; темп. наружного воздуха 7°CDB, 6°CWB; эквивалентная длина труб с хладагентом: 5 м"]
["","","","","","(3) - Электрические параметры см. в отдельных чертежах"]