{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTJ-AB"]
[]
[]
[]
[]
["","","","","","FTXTJ30A2V1BB"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.024"]
["","Hагрев","","Ном.","кВт","0.024"]
["Корпус","Цвет","","","","Черный"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","305"]
["","","","Ширина","мм","900"]
["","","","Глубина","мм","212"]
["Масса","Блок","","","кг","12"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","12.1"]
["","","","Средн.","м³/мин","8.8"]
["","","","Низк.","м³/мин","5.9"]
["","","","Тихая работа","м³/мин","4.9"]
["","","Hагрев","Выс.","м³/мин","12.3"]
["","","Нагрев","Средн.","м³/мин","7.8"]
["","","Hагрев","Низк.","м³/мин","6.5"]
["","","","Тихая работа","м³/мин","4.5"]
["Уровень звуковой мощности","Охлаждение","","","дБA","60"]
["","Отопление","","","дБA","60"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","43"]
["","","","Средн.","дБA","32"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","25"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","20"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","41"]
["","Нагрев","","Средн.","дБA","31"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","24"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","19"]
["Хладагент","ПГП","","","","675"]
["Подсоединение труб","Жидкость","","НД","мм","6.35"]
["","Газ","","НД","мм","9.5"]
["","Дренаж","","","","18"]
["Системы управления","Infrared remote control","","","","ARC488A4K"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Электропитание","Фаза","","","","1~"]
["","Частота","","","Гц","50"]
["","Напряжение","","","V","220-240"]