{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M / RXTM-N"]
[]
[]
[]
[]
["","","","","FTXTM30M2V1B / RXTM30N2V1B","FTXTM40M2V1B / RXTM40N2V1B"]
["Производительность по охлаждению","Мин.","","кВт","0.70","0.70"]
["","Макс.","","кВт","4.50","5.10"]
["","Ном.","","кВт","3.00","4.00"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","366","542"]
["","EER","","","4.10","3.71"]
["","COP","","","5.34","5.37"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A"]
["","","Нагрев","","A","A"]
["Теплопроизводительность","Ном.","","кВт","3.20","4.00"]
["","Мин.","","кВт","0.80","0.80"]
["","Макс.","","кВт","6.70","7.20"]
["Примечания","","","","(1) - Электрические параметры см. в отдельных чертежах","(1) - Электрические параметры см. в отдельных чертежах"]
["","","","","(2) - Охлаждение: T2: темп. в помещении 26,6°C сух.т., 19,4°C вл.т., темп. наружного воздуха 48°C сух.т. [БТЕ/ч/Вт]","(2) - Охлаждение: T2: темп. в помещении 26,6°C сух.т., 19,4°C вл.т., темп. наружного воздуха 48°C сух.т. [БТЕ/ч/Вт]"]
["","","","","(3) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м.","(3) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]