{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S"]
[]
[]
[]
[]
["","","","","","FTXTM30S2V1B","FTXTM40S2V1B"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.035","0.053"]
["","Hагрев","","Ном.","кВт","0.039","0.06"]
["Корпус","Цвет","","","","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","295","299"]
["","","","Ширина","мм","778","998"]
["","","","Глубина","мм","272","292"]
["Масса","Блок","","","кг","10","15"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","11.5","15.1"]
["","","","Средн.","м³/мин","7.5","9.2"]
["","","","Низк.","м³/мин","5.2","5.6"]
["","","","Тихая работа","м³/мин","4.2","4.8"]
["","","Hагрев","Выс.","м³/мин","11.6","17"]
["","","Нагрев","Средн.","м³/мин","7.3","10"]
["","","Hагрев","Низк.","м³/мин","4.7","6"]
["","","","Тихая работа","м³/мин","4","5.1"]
["Уровень звуковой мощности","Охлаждение","","","дБA","60","60"]
["","Отопление","","","дБA","60","60"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","45","46"]
["","","","Средн.","дБA","33","32"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","25","24"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","21","20"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","45","46"]
["","Нагрев","","Средн.","дБA","31","31"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","22","22"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","19","19"]
["Хладагент","ПГП","","","","675","675"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35"]
["","Газ","","НД","мм","9.5","9.5"]
["","Дренаж","","","","18","18"]
["Системы управления","Инфракрасный пульт ДУ","","","","ARC466A83","ARC466A83"]
["","Проводной пульт дистанционного управления","","","","BRC073A1","BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Электропитание","Фаза","","","","1~","1~"]
["","Частота","","","Гц","50","50"]
["","Напряжение","","","V","220-240","220-240"]