{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":10,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N / RXZ-N"]
[]
[]
[]
[]
["","","","","FTXZ25NV1B / RXZ25NV1B","FTXZ25NV1B / RXZ25NV1B9","FTXZ35NV1B / RXZ35NV1B","FTXZ35NV1B / RXZ35NV1B9","FTXZ50NV1B / RXZ50NV1B9","FTXZ50NV1B / RXZ50NV1B"]
["Холодопроизводительность","Мин.","","кВт","0.6","0.6","0.6","0.6","0.6"]
["","Макс.","","кВт","3.9","3.9","5.3","5.3","5.8"]
["","Ном.","","кВт","2.5","2.5","3.5","3.5","5.0"]
["Подсоединения труб","Жидкость","НД","мм","6.35","6.35","6.35","6.35","6.35"]
["","Газ","НД","мм","9.5","9.5","9.5","9.5","9.5"]
["Номинальная эффективность","Годовое потребление энергии","","kWh","205","205","330","330","550"]
["","EER","","","6.10","6.10","5.30","5.30","4.55"]
["","COP","","","5.80","5.80","5.00","5.00","4.47"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A","A","A"]
["","","Нагрев","","A","A","A","A","A"]
["Теплопроизводительность","Ном.","","кВт","3.6","3.6","5.0","5.0","6.3"]
["","Мин.","","кВт","0.6","0.6","0.6","0.6","0.6"]
["","Макс.","","кВт","7.5","7.5","9.0","9.0","9.4"]
["Примечания","","","","(1) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(1) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(1) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(1) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(1) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(1) - 230 В"]
["","","","","(2) - 220 В","(2) - 220 В","(2) - 220 В","(2) - 220 В","(2) - 220 В","(2) - 240В"]
["","","","","(3) - 230 В","(3) - 230 В","(3) - 230 В","(3) - 230 В","(3) - 230 В"]
["","","","","(4) - 240В","(4) - 240В","(4) - 240В","(4) - 240В","(4) - 240В"]
["Холодопроизводительность","Мин.","","кВт","","","","","","0.6"]
["","Ном.","","кВт","","","","","","5.0"]
["","Макс.","","кВт","","","","","","5.8"]
["Теплопроизводительность","Мин.","","кВт","","","","","","0.6"]
["","Ном.","","кВт","","","","","","6.3"]
["","Макс.","","кВт","","","","","","9.4"]
["Номинальная эффективность","EER","","","","","","","","4.55"]
["","COP","","","","","","","","4.47"]
["","Годовое потребление энергии","","кВтч","","","","","","550"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","","","","","","A"]
["","","Нагрев","","","","","","","A"]
["Подсоединение труб","Газ","НД","мм","","","","","","9.5"]
["","Жидкость","НД","мм","","","","","","6.35"]
["Охлаждение помещений","Класс энергоэффективности","","","","","","","","A+++"]
["","Производительность","Pрасч.","кВт","","","","","","5.00"]
["","SEER","","","","","","","","8.60"]
["","Годовое потребление энергии","","кВтч/г","","","","","","203"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","","","","","","A+++"]
["","Производительность","Pрасч.","кВт","","","","","","5.60"]
["","SCOP/A","","","","","","","","5.50"]
["","Годовое потребление энергии","","кВтч/г","","","","","","1427"]