{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Уровень звукового давления","Hагрев","","Выс.","дБ(A)","39","42","44"]
["","","","Тихая работа","дБ(A)","19","19","24"]
["","","","Низк.","дБ(A)","28","29","31"]
["","Охлаждение","","Тихая работа","дБ(A)","19","19","23"]
["","","","Низк.","дБ(A)","26","27","30"]
["","","","Выс.","дБ(A)","38","42","47"]
["","","","Ном.","дБ(A)","35","36","38"]
["","Охлаждение","","Ном.","дБ(A)","33","35","38"]
["Стандартные аксессуары","Фотокаталитический фильтр для очистки воздуха с функцией дезодорации","","","","1","1","1"]
["","Беспроводной пульт дистанционного управления","","","","1","1","1"]
["","Сухие батареи","","","","2","2","2"]
["","Держатель пульта дистанционного управления","","","","1","1","1"]
["","Крепежные винты внутреннего блока","","","","3","3","3"]
["","Монтажная пластина","","","","1","1","1"]
["Системы управления","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.5","9.5","9.5"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.030","0.030","0.030"]
["","Hагрев","","Ном.","кВт","0.030","0.030","0.030"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","54","57","60"]
["","Отопление","","","дБ(A)","56","57","59"]
["Размеры","Блок","","Ширина","мм","798","798","798"]
["","","","Глубина","мм","372","372","372"]
["","","","Высота","мм","295","295","295"]
["Корпус","Цвет","","","","Белый","Белый","Белый"]
["Масса","Блок","","","кг","15","15","15"]
["Вентилятор","Расход воздуха","Hагрев","Выс.","м³/мин","11.7","13.3","14.4"]
["","","","Низк.","м³/мин","6.7","6.9","7.7"]
["","","","Тихая работа","м³/мин","4.8","4.8","5.9"]
["","","Охлаждение","Низк.","м³/мин","5.3","5.6","6.6"]
["","","","Выс.","м³/мин","10.7","12.1","15.0"]
["","","","Тихая работа","м³/мин","4.0","4.0","4.6"]
["","","","Ном.","м³/мин","8.6","9.2","10.7"]
["","","Охлаждение","Ном.","м³/мин","7.5","8.4","9.2"]
["Power supply","Фаза","","","","1~","1~","1~"]
["","Наименование","","","","V1","V1","V1"]
["","Частота","","","Гц","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240"]
["Примечания","","","","","(1) - 220 В","(1) - 220 В","(1) - 220 В"]
["","","","","","(2) - 230 В","(2) - 230 В","(2) - 230 В"]
["","","","","","(3) - 240В","(3) - 240В","(3) - 240В"]
["","","","","","(4) - Передняя сторона теплообменника","(4) - Передняя сторона теплообменника","(4) - Передняя сторона теплообменника"]
["","","","","","(5) - Задняя сторона теплообменника","(5) - Задняя сторона теплообменника","(5) - Задняя сторона теплообменника"]