{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-A9"]
[]
[]
[]
[]
["","","","","","RXJ20A5V1B9","RXJ25A5V1B9","RXJ35A5V1B9","RXJ42A5V1B9","RXJ50A5V1B9"]
["Размеры","Блок","","Высота","мм","552","552","552","734","734"]
["","","","Ширина","мм","840","840","840","954","954"]
["","","","Глубина","мм","350","350","350","408","408"]
["Масса","Блок","","","кг","32","32","32","49","49"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","-10","-10","-10","-10","-10"]
["","","","Макс.","°CDB","50","50","50","50","50"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-21","-21","-21","-21","-21"]
["","","","Макс.","°CWB","18","18","18","18","18"]
["Уровень звукового давления","Охлаждение","","Ном.","дБA","46","46","49","48","48"]
["","Hагрев","","Ном.","дБA","47","47","49","48","49"]
["Хладагент","Тип","","","","R-32","R-32","R-32","R-32","R-32"]
["","Заправка","","","кг","0.76","0.76","0.76","1.1","1.1"]
["","Заправка","","","tCO2Eq","0.52","0.52","0.52","0.75","0.75"]
["","ПГП","","","","675","675","675","675","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20","20","20","30","30"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","15","15","15","20","20"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1","1","1"]
["","Drain cap","","","","","","","3","3"]
["","Drain plug","","","","1","1","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50"]
["","Напряжение","","","В","220-240","220-240","220-240","220-240","220-240"]
["Примечания","","","","","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","(2) - Электрические параметры см. в отдельных чертежах","(2) - Электрические параметры см. в отдельных чертежах","(2) - Электрические параметры см. в отдельных чертежах","(2) - Электрические параметры см. в отдельных чертежах","(2) - Электрические параметры см. в отдельных чертежах"]
["","","","","","(3) - Содержит фторированные парниковые газы","(3) - Содержит фторированные парниковые газы","(3) - Содержит фторированные парниковые газы","(3) - Содержит фторированные парниковые газы","(3) - Содержит фторированные парниковые газы"]