{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":16,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-M"]
[]
[]
[]
[]
["","","","","","RXJ20M5V1B","RXJ25M5V1B","RXJ35M5V1B","RXJ50MV1B","RXJ50M2V1B","RXJ20M2V1B (Archived)","RXJ20M3V1B (Archived)","RXJ25M2V1B (Archived)","RXJ25M3V1B (Archived)","RXJ35M2V1B (Archived)","RXJ35M3V1B (Archived)"]
["Вентилятор","Расход воздуха","Охлаждение","Сверхнизкий","м³/мин","","","","38.5","","29.3","","29.3","","29.3"]
["","","Нагрев","Сверхнизкий","м³/мин","","","","34.3","","25.6","","25.6","","25.6"]
["","","","Вентилятор-=-Расход воздуха-=-Охлаждение-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","","","","1359","","1035","","1035","","1035"]
["","","Нагрев","Вентилятор-=-Расход воздуха-=-Нагрев-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","","","","1211","","904","","904","","904"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","550","550","550","735","735","550","550","550","550","550","550"]
["","","","Ширина","мм","765","765","765","825","825","765","765","765","765","765","765"]
["","","","Глубина","мм","285","285","285","300","300","285","285","285","285","285","285"]
["Масса","Блок","","","кг","32","32","32","44","44","34","32","34","32","34","32"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","","","","620","","760","","760","","760"]
["","","Нагревание","Самый низкий","об/мин","","","","620","","740","","740","","740"]
["Компрессор","Type","","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Макс.","°C сух.т.","46","46","46","46","46","46","46","46","46","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Макс.","°CWB","18","18","18","18","20","18","18","18","18","18","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","","","","48","48","46","","46","","48"]
["","","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБA","46","46","49","","","","46","","46","","49"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","","","","","45"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","","","","48","48","47","","47","","48"]
["","","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБA","47","47","49","","","","47","","47","","49"]
["","","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","","","","","45"]
["Хладагент","Тип","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Заправка","","","кг","0.76","0.76","0.76","1.30","1.3","0.72","0.76","0.72","0.76","0.72","0.76"]
["","Заправка","","","tCO2Eq","0.52","0.52","0.52","0.9","0.88","0.5","0.52","0.5","0.52","0.5","0.52"]
["","ПГП","","","","675.0","675.0","675.0","675","675","675","675.0","675","675.0","675","675.0"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20","20","20","30","30","20","20","20","20","20","20"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","15.0","15.0","15.0","20","","15","15.0","15","15.0","15","15.0"]
["Стандартные аксессуары","Installation manual","","","","","","","1","","1","1","1","1","1","1"]
["","Drain plug","","","","","","","1","","1","1","1","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","","1~","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","","50","50","50","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240","220-240","","220-240","220-240","220-240","220-240","220-240","220-240"]
["Примечания","","","","","","","","(1) - 220 В","","(1) - 220 В","","(1) - 220 В","","(1) - 220 В"]
["","","","","","","","","(2) - 230 В","","(2) - 230 В","","(2) - 230 В","","(2) - 230 В"]
["","","","","","","","","(3) - 240В","","(3) - 240В","","(3) - 240В","","(3) - 240В"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Стандартные аксессуары","Refrigerant charge label","","","","","","","","","","1","","1","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","","","","","","1","","1","","1"]
["","General safety precautions","","","","","","","","","","1","","1","","1"]