{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":10,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-N9"]
[]
[]
[]
[]
["","","","","","RXP20N5V1B9","RXP25N5V1B9","RXP35N5V1B9","RXP50N5V1B9","RXP71N5V1B9 (Archived)"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","556","556","556","734","734"]
["","","","Ширина","мм","740","740","740","954","954"]
["","","","Глубина","мм","343","343","343","401","401"]
["Масса","Блок","","","кг","24","24","26","46","50"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10","-10","-10"]
["","","","Макс.","°C сух.т.","48","48","48"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15","-15","-15"]
["","","","Макс.","°CWB","18","18","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","46","46","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","47","47","48"]
["Хладагент","Тип","","","","R-32","R-32","R-32","R-32","R-32"]
["","Заправка","","","кг","0.55","0.55","0.70","0.9","1.15"]
["","Заправка","","","tCO2Eq","0.37","0.37","0.48"]
["","ПГП","","","","675.0","675.0","675.0","675","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20","20","20","30","30"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","12","12","12","20","20"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240"]
["Компрессор","Тип","","","","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Уровень звукового давления","Охлаждение","","Ном.","дБA","","","","47","52"]
["","Hагрев","","Ном.","дБA","","","","49","52"]
["Хладагент","Хладагент-=-Заправка-=-Экв. т CO2","","","Экв. т CO2","","","","0.61","0.78"]
["Стандартные аксессуары","Drain cap","","","","","","","3"]
["Диапазон энергоэффективности","","","","","","","","A+++ ~ D","A+++ ~ D"]
["Электропитание","Электропитание-=-Напряжение-=-В","","","В","","","","220-240","220-240"]
["Примечания","","","","","","","","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","","","","(2) - Электрические параметры см. в отдельных чертежах","(2) - Электрические параметры см. в отдельных чертежах"]
["","","","","","","","","(3) - Содержит фторированные парниковые газы","(3) - Содержит фторированные парниковые газы"]
["Стандартные аксессуары","Инструкции по установке","","","","","","","","1"]
["","Табличка с данными о заправке хладагентом","","","","","","","","1"]
["","Этикетки о фторированных парниковых газах на нескольких языках","","","","","","","","1"]
["","Сливная крышка","","","","","","","","3"]
["","Сливная пробка","","","","","","","","1"]