{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Уровень звукового давления","Hагрев","","Выс.","дБA","49","","","52"]
["","","","Низк.","дБA","46","","","49"]
["","Охлаждение","","Низк.","дБA","46","","","49"]
["","","","Выс.","дБA","49","","","52"]
["Стандартные аксессуары","Сливной патрубок","","","","1","","","1"]
["","Инструкции по установке","","","","1","","","1"]
["Хладагент","Charge","","","TCO2Eq","3.1","","","4.8"]
["","ПГП","","","","2,087.5","","","2,087.5"]
["","Заправка","","","кг","1.5","","","2.3"]
["","Тип","","","","R-410A","","","R-410A"]
["Подсоединение труб","перепад уровня","IU - OU","Макс.","м","20","","","20"]
["","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","","","0,02 (для длины труб свыше 10 м)"]
["Уровень звуковой мощности","Охлаждение","","","дБA","","","","65"]
["Compressor","Type","","","","Герметичный компрессор ротационного типа","","","Герметичный компрессор ротационного типа"]
["Размеры","Блок","","Ширина","мм","825","","","900"]
["","","","Глубина","мм","300","","","320"]
["","","","Высота","мм","735","","","770"]
["Масса","Блок","","","кг","48","","","71"]
["Power supply","Фаза","","","","1~","","","1~"]
["","Частота","","","Гц","50","","","50"]
["","Напряжение","","","V","220-240","","","220-240"]
["Примечания","","","","","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха","(1) - 220 В","","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха","(1) - 220 В"]
["","","","","","(2) - Содержит фторированные парниковые газы","(2) - 230 В","","(2) - Содержит фторированные парниковые газы","(2) - 230 В"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","735","735","","770","770"]
["","","","Ширина","мм","","825","825","","900","900"]
["","","","Глубина","мм","","300","300","","320","320"]
["Масса","Блок","","","кг","","48","48","","71","71"]
["Compressor","Type","","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","","-10","-10","","-10","-10"]
["","","","Макс.","°C сух.т.","","46","46","","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","","-15","-15","","-15","-15"]
["","","","Макс.","°CWB","","18","20","","18","20"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","","49","49","","52","52"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","","46","46","","49","49"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","","49","49","","52","52"]
["","","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","","46","46","","49","49"]
["Хладагент","Тип","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Заправка","","","кг","","1.5","1.5","","2.3","2.3"]
["","Заправка","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","ПГП","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","","30","30","","30","30"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","","20","20","","20","20"]
["Стандартные аксессуары","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Электропитание","Фаза","","","","","1~","1~","","1~","1~"]
["","Частота","","","Гц","","50","50","","50","50"]
["","Напряжение","","","V","","220-240","220-240","","220-240","220-240"]
["Примечания","","","","","","(3) - 240В","","","(3) - 240В"]
["Стандартные аксессуары","Drain socket","","","","","","1","","","1"]