{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTA-C"]
[]
[]
[]
[]
["","","","","","RXTA30C2V1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","605"]
["","","","Ширина","мм","930"]
["","","","Глубина","мм","376"]
["Масса","Блок","","","кг","42"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","800"]
["","","Нагревание","Самый низкий","об/мин","400"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10"]
["","","","Макс.","°C сух.т.","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-31"]
["","","","Макс.","°CWB","18"]
["Уровень звукового давления","Охлаждение","","Ном.","дБA","48"]
["","Hагрев","","Ном.","дБA","49.0"]
["Хладагент","Тип","","","","R-32"]
["","Заправка","","","кг","0.97"]
["","Хладагент-=-Заправка-=-Экв. т CO2","","","Экв. т CO2","0.66"]
["","ПГП","","","","675.0"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","15.0"]
["Стандартные аксессуары","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["Диапазон энергоэффективности","","","","","A+++ ~ D"]
["Электропитание","Фаза","","","","1~"]
["","Частота","","","Гц","50"]
["","Электропитание-=-Напряжение-=-В","","","В","220-240"]
["Примечания","","","","","(1) - Содержит фторированные парниковые газы"]
["","","","","","(2) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","(3) - Электрические параметры см. в отдельных чертежах"]