{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTA-N"]
[]
[]
[]
[]
["","","","","","RXTA30N2V1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","551"]
["","","","Ширина","мм","763"]
["","","","Глубина","мм","312"]
["Масса","Блок","","","кг","38"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","450"]
["","","Нагревание","Самый низкий","об/мин","360"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10"]
["","","","Макс.","°C сух.т.","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-25"]
["","","","Макс.","°CWB","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБA","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБA","49"]
["Хладагент","Тип","","","","R-32"]
["","Заправка","","","кг","1.1"]
["","Заправка","","","tCO2Eq","0.74"]
["","ПГП","","","","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","15"]
["Стандартные аксессуары","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["Электропитание","Фаза","","","","1~"]
["","Частота","","","Гц","50"]
["","Напряжение","","","V","220-240"]