{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":10,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RYN-L"]
[]
[]
[]
[]
["","","","","","RYN20LV1B","RYN25LV1B","RYN35LV1B","RYN50LV1B","RYN60LV1B"]
["Хладагент","Charge","","","TCO2Eq","","1.7"]
["","ПГП","","","","","2,087.5"]
["","Заправка","","","кг","","0.80"]
["","Тип","","","","","R-410A"]
["Подсоединения труб","Перепад уровней","IU - OU","Макс.","м","","5"]
["Компрессор","Тип","","","","","Ротационный"]
["Размеры","Блок","","Ширина","мм","","700"]
["","","","Глубина","мм","","250"]
["","","","Высота","мм","","521"]
["Масса","Блок","","","кг","","29"]
["Power supply","Фаза","","","","","1~"]
["","Частота","","","Гц","","50"]
["","Напряжение","","","V","","220-240"]
["Примечания","","","","","","(1) - Все технические характеристики могут быть изменены изготовителем без предварительного уведомления."]
["","","","","","","(2) - Содержит фторированные парниковые газы"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","494","","521","651","753"]
["","","","Ширина","мм","600","","700","855","855"]
["","","","Глубина","мм","245","","250","328","328"]
["Масса","Блок","","","кг","25","","31","49","50"]
["Компрессор","Тип","","","","Вращение","","Вращение","Вращение","Вращение"]
["Хладагент","Тип","","","","R-410A","","R-410A","R-410A","R-410A"]
["","Заправка","","","кг","0.65","","0.85","1.45","1.65"]
["","Заправка","","","tCO2Eq","1.7","","1.8","3","3.4"]
["","ПГП","","","","2087.5","","2087.5","2087.5","2087.5"]
["Электропитание","Фаза","","","","1~","","1~","1~","1~"]
["","Частота","","","Гц","50","","50","50","50"]
["","Напряжение","","","V","220-240","","220-240","220-240","220-240"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","","","19","19","19"]
["","","","Макс.","°C сух.т.","","","46","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","","","-9","-9","-9"]
["","","","Макс.","°CWB","","","18","18","18"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","","","12","15","15"]
["Подсоединения труб","перепад уровня","IU - OU","Макс.","м","","","5","8","8"]