{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-A"]
[]
[]
[]
[]
["","","","","","RZAG35A2V1B","RZAG50A2V1B","RZAG60A2V1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","734","734","734"]
["","","","Ширина","мм","870","870","870"]
["","","","Глубина","мм","373","373","373"]
["Масса","Блок","","","кг","52","52","52"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Уровень звуковой мощности","Охлаждение","","","дБA","62.0","63.0","64.0"]
["","Отопление","","","дБA","62.0","63.0","64.0"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБA","48.0","49.0","50.0"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБA","48.0","49.0","50.0"]
["Хладагент","Тип","","","","","R-32"]
["","Заправка","","","кг","1.55","1.55","1.55"]
["","ПГП","","","","675.0","675.0","675.0"]
["","Заправка","","","tCO2Eq","1.05","1.05","1.05"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.50","12.7","12.7"]
["","Длина трубы","Макс.","НБ - ВБ","м","50","50","50"]
["","","Система","Без заправки","м","30","30","30"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 30 м)","0,02 (для длины труб свыше 30 м)","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","30.0","30.0","30.0"]
["Стандартные аксессуары","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Электропитание","Фаза","","","","","1~"]
["","Частота","","","Гц","50","50","50"]
["","Напряжение","","","V","","220-240"]