{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":13,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-NV1"]
[]
[]
[]
[]
["","","","","","RZAG71N7V1B","RZAG71N2V1B","RZAG100N7V1B","RZAG100N2V1B","RZAG125N7V1B","RZAG125N2V1B","RZAG140N7V1B","RZAG140N2V1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","870","870","870","870","870","870","870","870"]
["","","","Ширина","мм","1100","1100","1100","1100","1100","1100","1100","1100"]
["","","","Глубина","мм","460","460","460","460","460","460","460","460"]
["Масса","Блок","","","kg","81","81","85","85","95","95","95","95"]
["Компрессор","Тип","","","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Макс.","°CDB","52","52","52","52","52","52","52","52"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Макс.","°CWB","18","18","18","18","18","18","18","18"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","64","64","66","66","69","69","70","70"]
["","Отопление","","","дБ(A)","","","","","68 (1)","68 (1)","71 (1)","71 (1)"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","46","46","47","47","49","49","50","50"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","48","48","50","50","52","52","52","52"]
["Хладагент","Тип","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Заправка","","","kg","3.2","3.20","3.2","3.20","3.7","3.70","3.7","3.70"]
["","ПГП","","","","675","675","675","675","675","675","675","675"]
["","Заправка","","","tCO2Eq","2.16","2.16","2.16","2.16","2.5","2.50","2.5","2.50"]
["Подсоединение труб","Жидкость","","НД","мм","10","10","10","10","10","10","10","10"]
["","Газ","","НД","мм","15.9","15.9","15.9","15.9","15.9","15.9","15.9","15.9"]
["","Длина трубы","Макс.","НБ - ВБ","м","55","55","85","85","85","85","85","85"]
["","","Система","Равносильно","м","75","75","100","100","100","100","100","100"]
["","","","Без заправки","м","40","40","40","40","40","40","40","40"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","См. инструкции по установке","См. инструкции по установке","См. инструкции по установке","См. инструкции по установке","См. инструкции по установке","См. инструкции по установке","См. инструкции по установке","См. инструкции по установке"]
["","перепад уровня","IU - OU","Макс.","м","30","30","30","30","30","30","30","30"]
["","","IU - IU","Макс.","м","0.5","0.5","0.5","0.5","0.5","0.5","0.5","0.5"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1","1"]
["","Peel off F-gas label","","","","1","1","1","1","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2","2","2","2","2"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50","50","50","50"]
["","Напряжение","","","В","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Ток — 50 Гц","Макс. ток предохранителя (MFA)","","","A","20","20","32","32","32","32","32","32"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Примечания","","","","","","","","","(1) - Согласно ENER Lot 21","(1) - Согласно ENER Lot 21","(1) - Согласно ENER Lot 21","(1) - Согласно ENER Lot 21"]